Seizmik® Halo-R Rearview Mirror with ABS Trim
			
Part #		Clamp Size	Fitment	
18053	Can-Am Defender Header Panel	Can-Am Defender	
18055		1.625” w/shims for 1.5"
	Honda Pioneer 500/700; Yamaha Wolverine, Viking and YXZ	
18056	1.75”	Round tube Polaris Ranger; Polaris RZR; John Deere Gator; Arctic Cat Wildcat; Yamaha Rhino	
18057	2.0” w/shims for 1.875” 	Round tube Can-Am; Kubota; Kawasaki; Honda 1000	
18058	Polaris Pro-Fit Header Panel	Pro-Fit Ranger	

Features:

•	Two Ball Joints—Maximizes range of adjustment.
•	High Impact ABS Plastic Housing—Resists damage.
•	Shatter Resistant Safety Glass—For maximum safety.
•	Convex Mirror Surface—Wider viewing range and image stabilization.
•	Built Tough—Heavy duty steel clamp with low mass design for maximum strength and durability.
•	Impact Resistant ABS Bezel—Protects and secures mirror glass and allows for easy glass replacement.
•	Color Kits Available—Customize your look (ships with grey bezel and back logo).
•	Seizmik Design—Styled to compliment all SEIZMIK side view mirrors.
•	UNLIMITED LIFETIME WARRANTY

Updated /2/8/20

Individual Product Packaging:

Length:	11.91 in
Width:		6.93 in
Height:	2.157 in
Weight:	23 oz

Updated 2/7/20